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3.7-4.2GHz 6W VTX Video Transmitter Shrimp B

Key Features
- None standard frequency from 3.7G to 4 .2G for less congestion .
- Designed for long-range flights , up to 6W transmitting power, and provide multi-level adjustment.
- Efficient PA and power calibration to ensure power consistency across all channels .
- Customized digital PLL circuit , chip level integration , no frequency drift.
- Aluminum alloy three-layer shell structure and large
centrifugal fan provide sufficient heat dissipation to ensure stable output of transmitting power.
[bookmark: _GoBack]- 32 channels supports band switching within the 3.7–4 .2GHz range .

General Characteristics
	Frequency band
	3700-4320 MHz
	Output power
	25mW/200mW/1W/6W

	Channel
	32 CH
	Frequency precision
	±200KHz (Typ.)

	Modulation type
	FM
	Power Supply
	DC 7-36V

	Frequency control
	PLL
	Video input level
	1V±0.2Vp-p (typ.)

	Control Protocol
	IRC Tramp
	S/N(For ±3MHz)
	>55dBc

	Antenna
	SMA 50 Ohms
	Operating Temperature
	-10℃~+70℃

	Dimension
	44*28.6* 14.7mm
	Weight
	25.3g



Frequency table
	BAND
	CH1
	CH2
	CH3
	CH4
	CH5
	CH6
	CH7
	CH8

	BANDA
	3700
	3720
	3740
	3760
	3780
	3800
	3820
	3840

	BAND b
	3860
	3880
	3900
	3920
	3940
	3960
	3980
	4000

	BAND C
	4020
	4040
	4060
	4080
	4100
	4120
	4140
	4160

	BAND d
	4180
	4200
	4220
	4240
	4260
	4280
	4300
	4320



RF Power
	Value
	25
	200
	1000
	5000

	Power level
	25mW
	200mW
	1W
	5W

	Gain
	14dBm
	23dBm±0.5
	30dBm±0.5
	38dBm±0.5
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Button Operation
	- Controlled using a single button , the button integrates RGB lighting , blue for band , red for channel , and green for power level.
- When there is no operation , the RGB LED blinks cyclically, the number of times the RGB blinks represents the current VTX status (when the green LED is always on , the VTX
enters PITMODE) .
- Long press the button to enter VTX setting , at this time the RGB lights are lit alternately, release the button under the corresponding color light to enter the corresponding function setting. At this time , short press the button to adjust the value .
For setup via the flight controller, connect the DATA pin and use the IRC Tramp protocol.


Attention

	Antenna must be connected before use! Otherwise there is a risk of damage to the product.
The product needs to be mounted reliably, avoiding vibration and high temperatures . The product has a built-in power filter, but still need to avoid excessive power supply interference .
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Wiring and Operation
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